{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["monFichier"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"monFichier","index":0,"n_rows":11,"n_cols":6,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Date","Pic journalier consommation (MW)","TempÃ©rature moyenne (Â°C)","TempÃ©rature rÃ©fÃ©rence (Â°C)","Estimation de puissance consommée :"]
["2017-02-24","70337.0","7.2","6.9","70337.0"]
["2016-12-03","72343.0","4.2","6.3","72343.0"]
["2015-05-08","49975.0","14.8","14.8","49975.0"]
["2012-08-12","43660.0","21.1","20.7","43660.0"]
["2019-04-08","64273.0","10.5","11.0","64268.0","dans le csv c'est 64268"]
["2017-04-16","50653.0","11.6","12.0","62803.0","deux résultats possibles : un 16/04/2017 l'autre en 16/04/2019 : les 2 sont-ils  \"justes\" ?"]
["2019-03-06","68945.0","10.6","7.6","68765.0","deux résultats possibles : un 06/03/2019 ligne 1064 et 06/03/2013 ligne 3255 (mêmes températures) … le premier est à 68765, le deuxième à 71564"]
["2019-12-24","60876.0","10.4","4.8","61001.0","dans le csv c'est 61001,0 ligne 771"]
["2018-01-12","76820.0","5.3","4.7","76820.0"]
["2016-07-11","55183.0","20.7","20.9","55183.0"]